Concrete/Mortar Mixer Machine

The tradition concrete mixers are mostly used to RCC Column, Beam & Roof etc.

This small mixer machine very suitable for small scale building mixing cement mortar for Brick work & Plastering work

An also used small scale industry like Ventilator, Precast post, Water filter, FC Wall Pannels making etc.

We can provide the solution equipment of this field.

**Dram Type Mobile Concrete/ Mortar Mixer Machine**

**The Feature:**

1. Easy operation

2. Easy moving in and out at job site

3. Low maintenance

4. 220volts electrical power operating

5. Low investment cost of this mixer

☞Mixer Type - Dram type

☞Mixing Capacity – 1cft /batch (Normal) 1cft /batch (mix)

45.50/batch (Normal) 68.25 Kg/ batch (mix)

☞Elevating Speed

(Dram Revolution Speed) - 32~35 RPM

☞Required Motor - KW 0.37(H.P. 0.5)

RPM-1425

Volts- 220/240

AMPS- 5.0

Phase -1

☞Machine Weight - 80kg



PVC Dram

R-9’-4” , H-30”

BEARRING

MOTOR PULI

R-1”

STATER WHEEL

R-1”

MOTOR

0.5 HP , 1425 RPM

V-BELT

A-57

WHEEL

R-5”

PLY WHEEL

R-8.1”

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Machine | E:\Cement Mixter Machine\100NIKON\machine.jpg | | | |
| Dram  Size r-9”, h-30”  (120 liter.) | | | E:\Cement Mixter Machine\100NIKON\drame.jpg | |
| Motor- KW 0.37(H.P. 0.5),  1425 RPM,  Volts 220/240,  AMPS 5.0,  Phase 1. | | | E:\Cement Mixter Machine\100NIKON\motor.jpg | |
| 1. Wheel r-8.5” 2. Wheel r-5” | | | ` E:\Cement Mixter Machine\100NIKON\while.jpg | |
| E:\Cement Mixter Machine\while 1  1.jpg | | E:\Cement Mixter Machine\Belt 1.jpg | | E:\Cement Mixter Machine\100NIKON\puli.jpg |